Page 47: Send check-in message to portal

Page 50: Signal strengths

* Turn on and off with +CIER

Page 137: Examples

MO = Mobile originated

+CSQ command returns signal strength (I think)

DTE = data terminal equipment

“The service availability indicator provides a way for the FA to wait until the ISU can start an SBD session without receiving continual notifications of changes in signal strength.”

“This command is used to transfer a binary SBD message from the FA to the single mobile originated buffer in the ISU. The mobile originated buffer can contain only one message at any one time.”

“In this form of the command, the Data Module will respond with a “READY” message, and will then expect the FA to supply binary data (corresponding to a complete SV Measurements IE as defined in P0770-ICD-001) plus checksum, using the same format, protocol and Command Responses as in the +SBDWB command.”